Scanning Micro-Opaque images with the Epson 4900 Photo Scanner:

1) Open Photoshop Elements

2) From the "File" menu, select "Import --> Epson Perfection 4990".  This launches the Epson Scan software.

3) In the Epson Scan window, make sure the following settings are set:
	- Mode: Professional Mode
	- Image Type: 24-bit Color
	- Resolution: 2400 dpi

4) Click "Preview".  A new preview window opens.

5a) In the preview window, use the mouse to draw a rectangle around one of the pages.  Click the "Zoom" button and a new, enlarged Preview will appear allowing you to see if that is the page you want.

5b) If this is the page you want, click "Scan" in the first Epson Scan window.  Proceed to Step 6.

5c) If this is NOT the page you want to scan, click on the "Preview" tab at the top of the Preview window and go back to Step 5a.

6) Click the "Scan" button in the Epson Scan window.

7) When scanning is complete (roughly 30 seconds), close the Epson Scan window.  (The Preview window will also close.)

8) You should now be back in the Photoshop Elements application.  From the "File" menu, select "Save".  Select "JPEG" as the file format and make sure the destination is your "My Documents" folder.  

9) Once you have saved your scan(s), you can go to any lab computer and view or print the document.  It will be in your Helios Home Directory if you saved it to "My Documents" on this workstation.